IEEE P802.21  
Media Independent Handover Services

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed Remedy for Comment #117 of the WG LB9 on IEEE P802.21.1/D01 draft | | | | |
| Date: 2016-01-20 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Hyeong-Ho Lee,  Hyunho Park | ETRI |  |  | [holee@etri.re.kr](mailto:holee@etri.re.kr)  [hyunhopark@etri.re.kr](mailto:hyunhopark@etri.re.kr) |

Abstract

This document contains proposed remedy for Comment #117 of the WG LB9 on IEEE P802.21.1 /D01 draft based on the LB9 comments file(DCN: 21-16-0008-01-SAUC).

**Proposed Remedy for Comment #117 of the WG LB9 on IEEE P802.21.1/D01 draft**

Comment #117: Assign appropriate one ("L", "R", or "L, R") to each of MIS commands (MIS\_Prereg\_Xfer, MIS\_N2N\_Prereg\_Xfer, MIS\_Prereg\_ready, and MIS\_CTRL\_Transfer) in Table 4 of page 31

Table 4—MIS commands for handover services

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **MIS command** | | **(L) ocal, (R) emote** | | **Comments** | | **Defined in** | |
| MIS\_Net\_HO\_Candidate\_Query | | R | | Network initiates handover and sends a list of suggested networks and associated points of attachment. | | 5.11.3 | |
| MIS\_MN\_HO\_Candidate\_Query | | R | | Command used by MN to query and obtain handover related information about possible candidate networks. | | 5.11.4 | |
| MIS\_N2N\_HO\_Query\_Resources | | R | | This command is sent by the serving MISF entity to the target MISF entity to allow for resource query. | | 5.11.5 | |
| MIS\_MN\_HO\_Commit | | R | | Command used by MN to notify the serving net- work of the decided target network information. | | 5.11.6 | |
| MIS\_Net\_HO\_Commit | | R | | Command used by the network to notify the MN of the decided target network information. | | 5.11.7 | |
| MIS\_N2N\_HO\_Commit | | R | | Command used by a serving network to inform a target network that an MN is about to move toward that network, initiate context transfer (if applicable), and perform handover preparation. | | 5.11.8 | |
| MIS\_MN\_HO\_Complete | | R | | Notification from MISF of the MN to the target or source MISF indicating the status of handover completion. | | 5.11.9 | |
| MIS\_N2N\_HO\_Complete | | R | | Notification from either source or target MISF to the other (i.e., peer) MISF indicating the status of the handover completion. | | 5.11.10 | |
| MIS\_Net\_HO\_Bcst\_Commit | | R | | Command used by the network to notify the specific group of MNs of the decided target network information. | | 5.11.11 | |
| MIS\_Prereg\_Xfer | | R | | Transport parameters and link layer frames. | | 5.11.12 | |
| MIS\_N2N\_Prereg\_Xfer | | R | | Transport link layer frames between the SPoS and the TPos. | | 5.12.1 | |
| MIS\_Prereg\_Ready | | R | | Check readiness of preregistration on a target link. | | 5.11.13 | |
| MIS\_CTRL\_Transfer | | R | | Deliver control message encapsulated by the MIS header | | 5.11.14 | |