|  |
| --- |
| Chapter 7.3.5 Association-specific attributes |
| Date: 2017-12-12 |
| **Authors:**  |
| Name  | Affiliation  | Phone  | Email  |
| Max Riegel | Nokia |  | maximilian.riegel@nokia.com |
|  |  |  |  |
|  |  |  |  |
| **Notice:**This document does not represent the agreed view of the OmniRAN TG It represents only the views of the participants listed in the ‘Authors:’ field above. It is offered as a basis for discussion. It is not binding on the contributor, who reserve the right to add, amend or withdraw material contained herein.  |
| **Copyright policy:**The contributor is familiar with the IEEE-SA Copyright Policy <<http://standards.ieee.org/IPR/copyrightpolicy.html>>.  |
| **Patent policy:** The contributor is familiar with the IEEE-SA Patent Policy and Procedures:<[http://standards.ieee.org/guides/bylaws/sect6-7.html#6](http://standards.ieee.org/guides/bylaws/sect6-7.html)> and <[http://standards.ieee.org/guides/opman/sect6.html#6.3](http://standards.ieee.org/guides/opman/sect6.html)>. |

Abstract

This document proposes a revision to the chapter 7.3.5

* Alignment of content with chapter 8.1.1

# Functional Decomposition and Design

## Association

### Association-specific attributes

#### Access link

An access link is established through the association process. It is defined through:

* {1} Link-ID: Unique link identifier
* {1} LinkConfig: configuration values of the link

#### TE

* {1+} SupportedLinkCapabilities: possible link configuration
* {1+} SupportedSecurityCapabilities: possible security modes
* {1+} SupportedQosCapabilities: possible QoS configuration

#### NA

* {1+} AllowedLinkCapabilities: allowed link configuration
* {1+} AllowedSecurityCapabilities: allowed security modes
* {1+} AllowedQosCapabilities: allowed QoS configurations
* {1} PreferredLinkProfile: desired link configuration attributes
* {1} PreferredSecurityProfile: desired security mode
* {1} PreferredQosProfile: desired QoS mode

### Association-specific basic functions