IEEE P802.11
Wireless LANs

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| CR non HT definition |
| Date: 2017-05-02 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Matthew Fischer | Broadcom |  |  | Matthew.fischer@broadcom.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

 |

Abstract

Comment resolution with proposed changes to TGax D1.2 for a CID that was already resolved once, as justification for dealing with a necessary, but missing change to the baselinen definition of non-HT PPDU.

The CID to be reresolved is:

9228

The proposed changes on this document are based on TGax Draft 1.2.

**REVISION NOTES:**

**R0**:

Initial

**END OF REVISION NOTES**

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

**CIDs**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 9228 | Tomoko Adachi | 3.05 | 3.2 | The definition of HE PPDU should be included. | Add a definition of HE PPDU in clause 3.2. | REVISED (PHY: 2017-03-19 15:45:31Z)11ax editor, please see the discussion for instructions in doc IEEE802.11-17/0330r2 and 11-17/0775r0 |

**Discussion:**

The baseline definition of non-HT does not yet include HE PPDU.

**Proposed Changes to Draft Text of TGax D1.2:**

***TGax editor: modify subclause 3.2 Definitions specific to IEEE Std 802.11, as shown:***

**3.2 Definitions specific to IEEE Std 802.11**

**non-high-throughput (non-HT):** A modifier meaning the logical combination of not high throughput (HT) and not very high throughput (VHT) and not high efficiency (HE).

**End of proposed changes.**