IEEE P802.11
Wireless LANs

|  |
| --- |
| Suggested comment resolution for CID 2525 on REMmd D2.0 |
| Date: 2019-07-13 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Marc Emmelmann | Self | Berlin, Germany |  | emmelmann@ieee.org |
| Hitoshi Morioka | SRC Sorftware | Fukuoka, Japan |  | hmorioka@src-soft.com |
| Hiroshi Mano | KDTI | Tokyo, Japan |  | mano@koden-ti.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

# Abstract

This submission presents a suggested comment resolution for CID(s) 2525 on REVmd D2.0

**Note – please do NOT consider this document. It has been merged in 11-19/1278 to address several related comments.**

Table of Contents

[Abstract 1](file:////Users/mem/Documents/Privat/Projects/802.11-TGm/REVmd-D2-Fils_comments/11-19-1260-00-000m-Suggested%20comment%20resolution%20for%20CID%202525%20on%20REMmd%20D2.0.docx#_Toc14081041)

[Comment 3](#_Toc14081042)

[Discussion 3](#_Toc14081043)

[Proposed Resolution 3](#_Toc14081044)

# Comment

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CID** | **LB** | **Draft** | **Page** | **Line** | **Clause** | **Comment** | **Proposed Change** |
| 2525 | 236 | 2 |  |  | 9.4.2.186 | "fast initial link setup category (FILSC): A value that indicates the priority category of the station (STA) for fast initial link setup" is confusing. FILSC is just DILS by another name, and should be called that | In 3.2: delete the FILSC definition and add a DILS definition "differentiated initial link setup (DILS): A mechanism for restricting fast initial link setup (FILS) to certain categories of stations."In 3.4: delete the FILSC expansion and add DILS with expansion "differentiated initial link setup"In 9.4.2.186 (multiple), 11.46.5.3: change "FILSC Type" to "DILS Type"In 9.4.2.186: change "The Differentiated FILS Time field contains an unsigned integer that specifies the time duration for the validity of the MAC Address Filter field or the FILS User Priority field" to "The Differentiated FILS Time field contains an unsigned integer that specifies the time duration for the DILS restrictions (see 11.46.5.3)"Finally, in 9.4.2.186 (multiple), 11.45.5 (multiple): change "Differentiated FILS Time" to "DILS Duration" |

# Discussion

CID 338 removed most of the remaining "FILSC" concept, but it remains in clause 9 terminology and definition. Corresponding clean-ups have been addressed as part of CID 2247. Therein, text has been deleted, for which this comment suggests changes.

The suggested resolution below is a copy of the suggested resolution for CID 2247 as contained in 19/1257.

# Proposed Resolution

REVISED

Delete "fast initial link setup category (FILSC)" definition in subclause 3.2.

Delete FILSC acronym in subclause 3.4.

In 9.4.2.186, replace "FILS Type" field name with "DILS Fields Present" (4 occurences, including the figure caption), and also in 11.46.5.3 (1 occurrence).