IEEE P802.11 Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed text for 4.4 | | | | |
| Date: 2021-02-26 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Chong Han | pureLiFi |  |  | chong.han@purelifi.com |
| Nikola Serafimovski |  |  | [nikola.serafimovski@purelifi.com](mailto:nikola.serafimovski@purelifi.com) |
| Stephan Berner |  |  | [stephan.berner@purelifi.com](mailto:stephan.berner@purelifi.com) |
| Mostafa Afgani |  |  | [Mostafa.afgani@purelifi.com](mailto:Mostafa.afgani@purelifi.com) |
| Tamas Weszely |  |  | [Tamas.weszely@purelifi.com](mailto:Tamas.weszely@purelifi.com) |

Abstract

This document provides text to be incorporated in the TGbb draft for the sub-clause 4.4.

History

r2-r3: follow the IEEE 802.11 style making changes on existing text. Texts that require changes are mentioned and listed in the standard. The changes are marked with underline.

r3-r4: change ‘not for facility’ to ‘not for LC’

### 4.4 Logical service interfaces

### 4.4.1 General

*Change the 2nd paragraph as follows:*

The complete set of IEEE 802.11 architectural services are as follows:

a) Authentication

b) Association

c) Deauthentication

d) Disassociation

e) Distribution

f) Integration

g) Data confidentiality

h) Reassociation

i) MSDU delivery

j) DFS (not for LC)

k) TPC (not for LC)

l) Higher layer timer synchronization (QoS facility only)

m) QoS traffic scheduling (QoS facility only)

n) Radio measurement (not for LC)

o) DSE (not for LC)

### 4.4.2 SS

*Change the 3rd paragraph as follows:*

The SS is as follows:

a) Authentication (not used when dot11OCBActivated is true)

b) Deauthentication (not used when dot11OCBActivated is true)

c) Data confidentiality (not used when dot11OCBActivated is true)

d) MSDU delivery

e) DFS (not for LC)

f) TPC (not for LC)

g) Higher layer timer synchronization (QoS facility only)

h) QoS traffic scheduling (QoS facility only)

i) Radio measurement (not for LC)

j) DSE (not for LC)

### 4.4.4 DSS

*Change the 3rd paragraph as follows:*

The services that comprise the DSS are as follows:

a) Association (not mesh facility)

b) Disassociation (not mesh facility)

c) Distribution

d) Integration

e) Reassociation (not mesh facility)

f) QoS traffic scheduling (QoS facility only)

g) DSE (not for LC)

h) Interworking with the DS (mesh facility only)

*Editor’s note: TBD. do we have to use ‘not LC facility’ for consistency? If so, need to define it in acronym.*