IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D0.3 CR for Section 36.3.18.4.3 and 36.3.19.2 | | | | |
| Date: 2021-3-02 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Wook Bong Lee | Samsung |  |  | wookbong.lee@samusng.com |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for the following comments on section 36.3.18.4.3 and 36.3.19.2 of TGbe D0.3:

* 2956, 2957

Baseline documents: TGbe D0.3.

Revisions:

* Rev 0: Initial version of the document. Use D0.3 as baseline spec text.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 2956 | 36.3.18.4.3 | 337 | Find a place to explicitely specify that "BPSK-DCM-DUP" is not allowed in EHT TB PPDU. | Clarify. | **Revised.**  Add following sentence in the Table 36-52. “N/A = not supported by the PPDU format.” |
| 2957 | 36.3.19.2 | 344 | Find a place to explicitely specify that "BPSK-DCM-DUP" is not allowed in 20/40MHz PPDU. | Clarify. | **Revised.**  Add following sentence in the Table 36-54. “N/A = not supported by the PPDU format.” |