IEEE P802.11
Wireless LANs

|  |
| --- |
| [CR on CID 1345] |
| Date: 2020-04-20 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Dongguk Lim | LG Electronics | 19, Yangjae-Daero 11 gil, Seoch-gu, Seoul, Korea |  | dongguk.lim@lge.com |
| Eunsung Park | LG Electronics |  |  | esung.park@lge.com |
| Jinyoung Chun | LG Electronics |  |  | jiny.chun@lge.com |
| Jinsoo Choi | LG Electronics |  |  | js.choi@lge.com |
| Bo Sun | ZTE |  |  |  |
| Brian Hart | Cisco |  |  |  |
| Edward Au | Huawei |  |  |  |

Abstract

This submission proposes resolutions for follwing 1 CID: 1345

Revisions:

* Rev 0: Initial version of the document.
* Rev 1:updated to reflect the offline discussion

## CID 1345

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 1345 | 227.03 | 36.3.11.5 | Text refers to "L\_DATARATE parameter in the TXVECTOR" but this is missing from 36.2.2 | Add L\_DATARATE to TX/RXVECTOR parameters in section 36.2.2 | Revised. Agree with commenter, in princlple. Since this parameter is used for the non-ht transmission, it should be described clearly. TGbe Editor: Incorporate the changes in https://mentor.ieee.org/802.11/dcn/21/11-21-0702-01-00be-CR-on-CID-1345.docx. |

Discussion :

As discussed in 11-21/635r2, instead of listing all paramters that is not present in EHT-PPDU in table 36-1, we decided to reuse the parameters described in table 27-1 for a DSSS, HR/DSSS, OFDM, ERP, HT, VHT or HE PPDU. But, since L\_DATALATE is missed in table 27-1, we can not use this parameter by referring the table 27-1 and also can not modify the table 27-1 in the TGbe. However, since it will be updated by working on the TGme when 11ax will be incorporated in the 11REVme, if the modification of table 27-1 will be done by the TGme, we can simply use this parameter as described in DCN 635r2.

To notify the waiting for updating the table 27-1, we can add the editor's note after table 36-1.

***TGbe editor: please add the editor’s note after Table 36-1—TXVECTOR and RXVECTOR parameters***

*Edtior’s Note: L\_DATARATE is not present in the table according to agreement in DCN 21/635r2 and currently missing because we are waiting for the update of clause 27*

**References:**

**[1] 802.11be D0.4**