IEEE P802.11Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed Resolutions to 11az LB253 CID-5424, 5425 | | | | |
| Date: 2021-07-14 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Qi Wang | Apple Inc. |  |  | qi\_wang2@apple.com |
| Tianyu Wu |  |  | tianyu@apple.com |

Abstract

This submission proposes the resolutions to 11az LB 253 CID-5424, 5425.

The page and line numbers for proposed changes refer to those in 11az Draft 3.0 [1].

**Introduction**

This submission proposes the resolutions to 11az LB 253 CID-5424, 5425.

The page and line numbers for proposed changes refer to those in 11az Draft 3.0 [1].

**Comments:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Page/Line | Clause | Comment | Proposed change | Resolution |
| 5424 | 225.00/28 | 27.3.18a | Clarify that LTF\_REP >=2 for Secure HE-LTF in HE Ranging NDP. | Change this sentence to: "The total number of HE-LTF symbols is the product of the number of LTF repetitions LTF\_REP, which is greater than or equal to 2, and" | Revised.  Agree with the commenter. However, the necessary changes are already made per the resolutions to CID-5189, 5192 included in submission 21/917r0.  TGaz editor: no action is needed. |
| 5425 | 227.00/22 | 27.3.18b | Clarify that LTF\_REP >=2 for Secure HE-LTF in HE TB Ranging NDP. | Add the following sentence to the end of this paragraph: "The number of repetitions is greater than or equal to 2. " | Revised.  Agree with the commenter. However, the necessary changes are already made per the resolutions to CID-5189, 5192 included in submission 21/917r0.  TGaz editor: no action is needed. |