IEEE P802.11
Wireless LANs

|  |
| --- |
| **TGbe CC36 Comment Resolutions for CID 4273 and 5139** |
| **Date:** 2021-09-14 |
| **Author(s):** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Name** | **Affiliation** | **Address** | **Phone** | **Email** |
| Jinyoung Chun | LG Electronics | 19, Yangjae-daero 11gil, Seocho-gu, Seoul 137-130, Korea  |   | jiny.chun@lge.com  |
| Dongguk Lim |  | dongguk.lim@lge.com |
| Eunsung Park |  | esung.park@lge.com |
| Insun Jang |  | insun.jang@lge.com |
| Jinsoo Choi |  | js.choi@lge.com |

Abstract

This submission proposes a resolution for 2 CIDs: CID 4273 and 5139

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe D1.0 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe D1.0 Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **PP.LL** | **Comment** | **Proposed Change** | **Resolution** |
| 4273 | 10.23.2.8 | 180.39 | Can Beamforming Report Poll frames be transmitted by EHT STAs (well HE STAs as well?). Seems we stopped calling them out from 11ax days. Please ensrue that they were not accidentally left out. | As in comment. | RejectedBeamforming Report Poll frame is used for VHT sounding, but this subclause includes all description about multiple frame transmission in an EDCA TXOP from VHT to EHT. And EHT STA keep backward complablity. So it’s better to keep the sentence. |
| 5139 | 10.23.2.8 | 180.32 | Add an (the) EHT TB PPDU after an (the) HE TB PPDU. | As in comment | RevisedTGbe editor: It was already resolved in Draft 1.01 by 21/493r1 (CID 2849). No further change is needed. |