IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed Comment Resolution for GEN CIDs (REVme D0.3) | | | | |
| Date: 2021-09-27 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Stephen MCCANN | Huawei Technologies Co., Ltd | Southampton, UK |  | [stephen.mccann@ieee.org](mailto:stephen.mccann@ieee.org) |

Abstract

This document proposes comment resolutions for the following CIDs:

500, 576 & 580

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| | **comments** | | | | | | | | | --- | --- | --- | --- | --- | --- | --- | --- | | **CID** | **Page** | **Clause** | **Resn Status** | **Comment** | **Proposed Change** | **Resolution** | **Owning Ad-hoc** | | 500 | 5150.49 | C.3 |  | "There is no reference to dot11STACivicLocation in main body of the standard. The same thing apply to dot11STACivicLocationType.  Furthermore, it seems that dot11STACivicLocationConfigTable is poorly defined and probably does not pass MIB compilation. In description of ""dot11RMCivicConfigured"", there is a reference to dot11STACivicLocationEntry. However, dot11STACivicLocationEntry is not defined anywhere." | As it says in the comment | Rejected: The comment fails to identify changes in sufficient detail so that the specific wording of the changes that will satisfy the commenter can be determined.  Notes:   1. this is a similar comment to REVmd CID 2304 in:   <https://mentor.ieee.org/802.11/dcn/18/11-18-0611-29-000m-revmd-wg-ballot-comments.xls>  and also REVmd CID 4706 in:  <https://mentor.ieee.org/802.11/dcn/19/11-19-2156-29-000m-revmd-sponsor-ballot-comments.xls>   1. In order for this CID to be resolved in another way, research needs to be performed to determine whether the two cited MIB variables be removed or not. | GEN | |
| | **comments** | | | | | | | | | --- | --- | --- | --- | --- | --- | --- | --- | | **CID** | **Page** | **Clause** | **Resn Status** | **Comment** | **Proposed Change** | **Resolution** | **Owning Ad-hoc** | | 576 | 317.02 | 4.5.9.2.2 |  | There is no definition for "ANQP Server", as it should be an "Advertisement Server" | Change "ANQP Server" to "Advertisement Server" and P277L21. Also change the term within Figure 4-20. | Revised. Change “ANQP Server” to “Advertisement server”. Also change the term within Figure 4-20. | GEN | | 580 | 5881.28 | R.2.1 |  | The term "access network server" is not defined. | Remove the phrase "(e.g., an access network server or an IEEE 802.21 Information Server)" from the cited sentence, as an advertisement server has been defined within the main body of the standard. These examples are not necessary. | Accepted | GEN | |