IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed Text for CR Part 2 | | | | |
| Date: 2022-01-19 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 111 West 33rd Street  New York, NY 10120  USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Rui Yang |  |  |
|  |  |  |  |  |

Abstract

This submission proposes the spec text for resolutions for the CID 2173, 2063, 2065. The baseline for this comment resolution document is 802.11bc Draft 2.1.

* Rev 0: first draft

***TGbc Editor: Please modify the text of 9.4.1.69 as follows (802.11bc D2.1).***

The EBCS Response Information List field contains one or more EBCS Response Info subfields. The format

of the EBCS Response Info subfield is shown in [Figure 9-144f (EBCS Response Info subfield format](#_bookmark69)).

54

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| EBCS  Response Info Control | Content ID | EBCS  Request Failure Code | Time To Termination | EBCS SP  Duration | EBCS SP  Interval |

Octets: 1 1 0 or 1 0 or 3 0 or 2 0 or 2

##### Figure 9-144f—EBCS Response Info subfield format [#2173, 2063]

***TGbc Editor: Please modify the text of B.4.38 as follows (802.11bc D2.1).[#2095]***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| \*EBCS4 | EBCS negotiation procedures | [11.55.4 (EBCS](#_bookmark217)  [negotia- tion proce- dure for associated](#_bookmark217) [STAs)](#_bookmark217) and [11.55.5 (EBCS](#_bookmark219)  [negotia- tion proce- dure for unassoci-](#_bookmark219) [ated STAs)](#_bookmark219) | CFAP AND CFEBCS: M CFSTAofAP AND EBCS1: M | Yes  No   N/A  |