IEEE P802.11
Wireless LANs

|  |
| --- |
| LB 275 CR for CID 19888 |
| Date: 2023-10-01 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Rui Yang | InterDigital |  |  | rui.yang@interdigital.com |
|  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

##### This submission present proposed resolutions for the following 1 CIDs:

##### 19888

##### The proposed changes are based on 802.11be/D4.0.

##### Revision history:

##### r0 – initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 19888 | 36.3.18 | 861.47 | "of EHT-SIG" should be "of the EHT-SIG field" | As in comment. | RevisedThe P.L for this comment should be 858.27. In D4.0 the article “the” has been added, but “field” after “EHT-SIG” is still missing.TGbe editor: please implement changes as shown in doc 11-23/1681r0 tagged as 19888.TGbe editor: In 802.11be D4.0, the same issue exists in several places listed below, where “EHT-SIG” is used as a noun:* P799, L59
* P896, L49/58/63
* P897, L2/8/12

Suggest adding “field” in those places, as well. |

***Tgbe editor: please make the following change in subclause 36.3.18***

NOTE—The number of EHT-LTF symbols in the EHT sounding NDP is indicated in the Number Of EHT-LTF Symbols field of the EHT-SIG field (#19888).