IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed resolution to CID 7179 | | | | |
| Date: 2024-05-14 | | | | |
| Author: | | | | |
| Name | Affiliation | Address | Phone | Email |
| Edward Au | Huawei Technologies | Ottawa, Ontario, Canada |  | [edward.ks.au@gmail.com](mailto:edward.ks.au@gmail.com) |

##### 

##### This submission present proposed resolutions for the following CID:

7179

##### The proposed changes are based on REVme D5.0.

##### Revision history:

##### R0 – Initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 7179 | D |  |  | In some parts of the spec FCC is for North America (e.g. DS5.1 in PICS "North America (FCC)") but in others it's just for the USA (e.g. dot11RegDomainsSupportedTable "FCC (USA and its territories(#296))"). One of the two must be incorrect | As it says in the comment |

***Discussion:***

There are two occurrences – one is DS5.1 and another is HRDS6.1 – with snapshots shown below.





The policies in the United States and Mexico are not exactly the same.

Suggest to duplicate the above PICS entries for United States FCC and Mexico IFT, respectively.

***Proposed resolution for CID 7179:***

Revised.

At 5028.13 for DS5.1, replace “North America (FCC)” with “United States and its territories (FCC)”.

At 5034.58, duplicate the entries of DS5.1.1, DS5.1.2, DS5.1.3, DS5.1.4, DS5.1.5, DS5.1.6, DS5.1.7, DS5.1.8, DS5.1.9, DS5.1.10, and DS5.1.11 for Mexico (IFT) as DS5.8.1, DS5.8.2, DS5.8.3, DS5.8.4, DS5.8.5, DS5.8.6, DS5.8.7, DS5.8.8, DS5.8.9, DS5.8.10, and DS5.8.11.

At 5061.25 for HRDS6.1, replace “North America (FCC)” with “United States and its territories (FCC)”.

At 5065.50, duplicate the entries of HRDS6.1.1, HRDS6.1.2, HRDS6.1.3, HRDS6.1.4, HRDS6.1.5, HRDS6.1.6, HRDS6.1.7, HRDS6.1.8, HRDS6.1.9, HRDS6.1.10, and HRDS6.1.11 for Mexico (IFT) as HRDS6.8.1, HRDS6.8.2, HRDS6.8.3, HRDS6.8.4, HRDS6.8.5, HRDS6.8.6, HRDS6.8.7, HRDS6.8.8, HRDS6.8.9, HRDS6.8.10, and HRDS6.8.11.