IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for 38.3.23 Transmit Specification on P802.11bn D0.1 | | | | |
| Date: 2025.03.30 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Genadiy Tsodik | Huawei Technologies |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission contains proposed comment resolutions to comments on P802.11bn D0.1.

3 out of 5 comments under 38.3.23 Transmit Specification are resolved.

# Revision Notes

|  |  |
| --- | --- |
| R0 | Initial revision |
| R1 | DCN is corrected |
|  |  |
|  |  |
|  |  |
|  |  |

## CID 953

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Page.  Line | Clause Number | Comment | Proposed Change | Resolution |
| 210.40 | 38.3.23.4.3 | Add Tx EVM requirement for UEQM based on first stream MCS's Tx EVM requirement | As in comment | REJECTED  According to motion 314, Transmit Specification should be defined for EQM only. |

## CID 954

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Page.  Line | Clause Number | Comment | Proposed Change | Resolution |
| 210.40 | 38.3.23.4.3 | Add Tx EVM requirement for new MCS levels | As in comment | REVISED  Agree with the commenter to add the Tx EVM requirements for new MCS levels. Details of the addition are shown in doc. 11-24/2021r0 |

## CID 1656

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Page.  Line | Clause Number | Comment | Proposed Change | Resolution |
| 210.07 | 38.3.23 | Define 38.3.23 Transmit specification | As in comment | REVISED  Agree with the commenter to define the missing transmit specification. Proposed text is shown in doc. 11-24/2021r0 |