**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Wireless Personal Area Networks |
| Title | **PAN ID Compression Table for Beacon, Data, Acknowledgement, Command frames** |
| Date Submitted | 11 Feb 2015 |
| Source | [][][PO Box 798 Los Gatos CA 95031] | Voice: [+1-408-395-7207]Fax: [ ]E-mail: ben.rolfe @ ieee.org] |
| Re: | 802.15.4 Revision Preparation  |
| Abstract | Submission to Maintenance standing committee: Proposed revised format and content for the PAN ID compression table and other related things. |
| Purpose | Promote useful work |
| Notice | This document has been prepared to assist the IEEE P802.24. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.24. |

PAN ID Compression for Beacon, Data, Acknowledgement, Command frames

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Frame Version | Source Address | Destination Address | PAN ID Comp | Frame Types | Source PAN ID | Dest PAN ID |
| 0b00 or 0b01 | Not Present | Not Present | 0 | Acknowledgement |  Not Present |  Not Present |
| Not Present | Not Present | 1 | Not valid for any frame type | NA | NA |
| Not Present | Present | 0 | Beacon, Data, Acknowledgment, Command | Not Present | Present |
| Not Present | Present | 1 | Not valid for any frame type | NA |  NA |
| Present | Not Present | 0 | Beacon, Data, Acknowledgment, Command |  Present |  Not Present |
| Present | Not Present | 1 | Not valid for any frame type | NA | NA |
| Present | Present | 0 | Beacon, Data, Acknowledgment, Command | Present | Present |
| Present | Present | 1 | Beacon, Data, Acknowledgment, Command |  Not Present |  Present |
| 0b10 | Not Present | Not Present | 0 | Beacon, Data, Acknowledgment, Command | Not Present | Not Present |
| Not Present | Not Present | 1 | Beacon, Data, Acknowledgment, Command | Not Present | Present |
| Not Present | Short or Extended | 0 | Beacon, Data, Acknowledgment, Command | Not Present |  Present |
| Not Present | Short | 1 | Not valid for any frame | NA |  NAA |
| Not Present | Extended | 1 | Beacon, Data, Acknowledgment, Command | Not Present | Not Present |
| Short or Extended | Not Present | 0 | Beacon, Data, Acknowledgment, Command |  Present | Not Present |
| Short | Not Present | 1 | Not valid for any frame | NA | NA |
| Extended | Not Present | 1 | Beacon, Data, Acknowledgment, Command | Not Present | Not Present |
| Short or Extended | Short or Extended | 0 | Beacon, Data, Acknowledgment, Command | Present | Present |
| Short | Short | 1 | Beacon, Data, Acknowledgment, Command | Not Present | Present |
| Short | Extended | 1 | Beacon, Data, Acknowledgment, Command | Not Present | Present |
| Extended  | Short | 1 | Beacon, Data, Acknowledgment, Command | Not Present | Present |
| Extended | Extended | 1 | Beacon, Data, Acknowledgment, Command | Not Present | Not Present |