IEEE P802.19
Wireless Coexistence

|  |
| --- |
| Proposed resolution to comment to clause 5.2.2.1 WSO subscription procedure |
| Date: 2012-09-18 |
| Author(s): |
| Name | Company | Address | Phone | email |
| Stanislav Filin | NICT |  |  | sfilin@nict.go.jp |
| Hiroshi Harada | NICT |  |  |  |

Abstract

This document is a submission to IEEE 802.19 TG1 proposing resolution to comment to clause 5.2.2.1 WSO subscription procedure.

**Notice:** This document has been prepared to assist IEEE 802.19. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

# Comment

WSO subscription procedure is not described, only figure is provided.

# Proposed resolution

*It is proposed to substitute the text in the clause 5.2.2.1 WSO subscription procedure by the text below.*

* + - 1. WSO subscription procedure

A CE shall perform the WSO subscription procedure when it has finished the WSO authentication procedure. An illustrative example of this procedure is shown in Figure 1. SubscriptionRequest and SubscriptionResponse messages are defined in clause 5.3 Messages.



Figure 1 WSO subscription procedure

After a CE has finished a WSO authentication procedure, it shall obtain WSO subscription information. After the WSO subscription information has been obtained, the CE shall generate a SubscriptionRequest message and shall send this SubscriptionRequest message to the CM that serves this CE. CE operation related to generating and sending a SubscriptionRequest message is specified in clause 6 CE Operation.

After the CM has received the SubscriptionRequest message from the CE, the CM shall perform WSO subscription, shall generate a SubscriptionResponse message and shall send this SubscriptionResponse message to the CE. CM operation related to WSO subscription, generating and sending a SubscriptionResponse message is specified in clause 7 CM Operation.

After the CE has received the SubscriptionResponse message from the CM, the CE shall process the SubscriptionResponse message. CE operation related to processing the SubscriptionResponse message is specified in clause 6 CE Operation.